{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["R Divider"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"R Divider","index":0,"n_rows":22,"n_cols":11,"rows_kept":22,"cut":false,"hidden":false,"merged":[]}
[null,"Resistor Divider"]
[null,"Electronic Design with Excel",null,null,null,null,null,null,null,null,"Enter"]
[null,null,null,null,null,null,null,null,null,null,"Calc"]
[]
[]
[]
[]
[]
[null,"ALT-F11 to see VBA Function."]
[]
[]
[]
["Input Signal"]
["Vs",10]
[]
["Resistor Divider"]
["R1",10000]
["R2",20000]
[]
["Gain and Output of Divider"]
["K Rdiv",{"$f":"K_Rdiv1(B17,B18)","v":0.66666666666666663}]
["Vo",{"$f":"B14*B21","v":6.6666666666666661}]